**MANUFACTURER SPECS**

* The all-new sixteen cubic foot AT16 Power Buggy with Track Drive provides excellent traction on grades, inclines, and soft soils. Providing more horsepower, more load carrying capacity and greater bucket volume than competitors; the new track buggy's rugged steel frame increases load weight and distributes the load across the entire frame, providing for smooth, even transport.
* Engine: Kohler Vert. Shaft (27hp) with Electric Start
* Payload: 2,500 lb. (1,135 kg)
* Dimensions (L x H): 102.5 in. x 65.25. in (260 x 166 cm)
* Length (with Platform Up): 92 in. (234 cm)
* Length (with Platform Down): 102.5 in. (260 cm)
* Dimensions (Width): 35.625 in. (90 cm)
* Wheelbase / Track Length: 119 in. (302 cm)
* Bucket Capacity: 16 cu. ft. (0.45 cu. m)
* Weight: 1475 lbs. (669 kg)
* Lift Cylinder: 2.5 in. Diameter (64 mm)
* Dump/Return Speed Empty: 7 Seconds
* Top Speed: Work: 4 mph (6 kph)
* Transport: 6 mph (10 kph)
* Fuel Capacity: 6 gal. (22.7 L)

**PRODUCT INFO**

* Huge 16 Cubic Foot Bucket Capacity
* Hydraulic Dump Action with 6" of ground clearance when fully dumped
* Heavy-Duty Poly Dump Bucket
* 27hp Kohler Engine
* Easy-To-Use Operator Controls
* Rubber Tracks
* Payload up to 2,500 lbs.
* All-New Steel Frame Design
* Two-Speed (Work and Transport) Hydrostatic Drive
* Two Work Lights
* 6 Gallon Fuel Tank