Specifications

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|   | MDL-5B | MDL-5H | MDL-8B | MDL-8H |
| Engine Brand/Model | B&S Vanguard OHV | Honda GX160 OHV | B&S Vanguard OHV | Honda GX240 OHV |
| Engine Horsepower | 5.5 hp (4.8 hp net) | 5.5 hp (4.8 hp net) | 8.0 hp (7.9 hp net) | 8.0 hp (7.9 hp net) |
| Oil Alert System | Standard | Standard | Standard | Standard |
| Torque Tube | Standard | Standard | Standard | Standard |
| Centrifugal Clutch | Standard | Standard | Standard | Standard |
| 7' Flexible Drive Shaft | Standard | Standard | Standard | Standard |
| Snap-On Auger Adaptor | Standard | Standard | Standard | Standard |
| Gear Reduction Ratio | 10:1 | 10:1 | 10:1 | 10:1 |
| RPM\* | 360 | 360 | 360 | 360 |
| Wheel Size | 8" | 8" | 10" | 10" |
| Wheel Type\*\* | Semi-pneumatic | Semi-pneumatic | Pneumatic | Pneumatic |
| Dry Shipping Weight | 125 lbs | 132 lbs | 147 lbs | 167 lbs |