|  |  |
| --- | --- |
| Capacity (pounds) | 12,000 |
| GVWR (pounds) | 15,700 |
| GAWR (pounds) | 14,000 |
| Avg. Weight (pounds) | 4,300 |
| Load Width (in) | 82" |
| Deck Height (in) unloaded | 25" |
| Std. Hitch Size (in) | 2-5/16" |
| Tongue/Gooseneck Length (ft) | 4'-7" |
| Safety Chain | 3/8 Gr. 43 |
| Parking Jack | 12K |
| Bolted-on Parking Jack | Y |
| Main Frame | 4x6 Tube |
| Deck Type | Dump Body |
| Deck Safety Lip | N/A |
| Deck Material | Steel |
| Added Stationary Deck | N/A |
| Ramps w/storage | S |
| Load Angle (degrees) | N/A |
| Dump Angle | 45 |
| Beavertail | N/A |
| Ramp Hold-Up | N/A |
| Ramp Spring Assist (off deck) | N/A |
| Ramp Spring Assist (off ground) | N/A |
| Stake Pockets | 10 |
| D-rings | 4 |
| Axle Capacity | 7K |
| No. of Axles | 2 |
| Axle Spread (in) | 34" |
| Hubs | EZ-Lube |
| Brake Size | 12" x 2" |
| Electric Brakes | Std. |
| Air Brakes | N/A |
| Wheels (size) | 16" |
| Wheel Bolt Pattern | 8-bolt |
| Tires | 235/85Rx16 |
| Tire Load Rating | E |
| Lights | LED |